# ?lamc3

Called from ?lamc1-?lamc5. Intended to force a and b to be stored prior to doing the addition of a and b.

## Syntax

val = slamc3( a, b )

val = dlamc3( a, b )

## Description

The routine is intended to force A and B to be stored prior to doing the addition of A and B, for use in situations where optimizers might hold one of these in a register.

## Input Parameters

a, b

  REAL for slamc3

  DOUBLE PRECISION for dlamc3

  The values a and b.

## Output Parameters

val

  REAL for slamc3

  DOUBLE PRECISION for dlamc3

  The result of adding values a and b.

Parent topic: Utility Functions and Routines